{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Phaseurs triphasés"],"not_rendered":{"charts":1,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Phaseurs triphasés","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[[20,10,21,13],[23,1,23,2],[23,3,23,4],[3,2,3,3],[3,4,3,5],[19,2,19,3],[19,4,19,5]]}
[]
[null,{"$f":"PI()","v":3.1415926535897931},null,null,null,null,null,null,null,null,"Principe des phaseurs appliqué à un système triphasé"]
[]
[null,null,"Vecteur tournant",null,"Projection horizontale"]
[null,null,0,0,{"$f":"C6","v":6.1257422745431001E-17},{"$f":"D6","v":1},null,1.4,1.4]
[null,0,{"$f":"COS(B6+PI()/2)","v":6.1257422745431001E-17},{"$f":"SIN(B6+PI()/2)","v":1},{"$f":"B6+1.4","v":1.4},{"$f":"D6","v":1},null,1.4,-1.4]
[]
[null,null,0,0,{"$f":"C9","v":-0.86602540378443882},{"$f":"D9","v":-0.49999999999999972},null,{"$f":"PI()/2+1.4","v":2.9707963267948965},0.03]
[null,{"$f":"B6+2*PI()/3","v":2.0943951023931953},{"$f":"COS(B9+PI()/2)","v":-0.86602540378443882},{"$f":"SIN(B9+PI()/2)","v":-0.49999999999999972},{"$f":"E6","v":1.4},{"$f":"D9","v":-0.49999999999999972},null,{"$f":"H8","v":2.9707963267948965},-0.03]
[]
[null,null,0,0,{"$f":"C12","v":0.86602540378443837},{"$f":"D12","v":-0.50000000000000044},null,{"$f":"PI()+1.4","v":4.5415926535897935},0.03]
[null,{"$f":"B9+2*PI()/3","v":4.1887902047863905},{"$f":"COS(B12+PI()/2)","v":0.86602540378443837},{"$f":"SIN(B12+PI()/2)","v":-0.50000000000000044},{"$f":"E6","v":1.4},{"$f":"D12","v":-0.50000000000000044},null,{"$f":"H11","v":4.5415926535897935},-0.03]
[]
[null,null,null,null,{"$f":"E12","v":1.4},{"$f":"MAX(F5,F8,F11)","v":1},null,{"$f":"3*PI()/2+1.4","v":6.11238898038469},0.03]
[null,null,null,null,{"$f":"E14","v":1.4},{"$f":"MIN(F6,F9,F12)","v":-0.50000000000000044},null,{"$f":"H14","v":6.11238898038469},-0.03]
[]
[null,null,null,null,null,null,null,{"$f":"2*PI()+1.4","v":7.6831853071795866},0.03]
[null,null,null,null,null,null,null,{"$f":"H17","v":7.6831853071795866},-0.03]
[]
[null,null,"θ tournant",null,"θ cosinus"]
[null,null,{"$f":"COS((B6/2+PI()/2))*0.35-0.09","v":-8.9999999999999969E-2},{"$f":"SIN((B6/2+PI()/2))*0.35+0.03","v":0.38},{"$f":"B6/2+1.4","v":1.4},-0.1,null,null,null,null,"À noter que pour les fins de cette animation l'axe des réels ℝ est ici tourné de 90° anti-horaire"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Pour les fins du cours \"Caractéristiques électriques des postes HT/MT\""]