{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Comp. sym à phaseurs"],"not_rendered":{"charts":1,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Comp. sym à phaseurs","index":0,"n_rows":27,"n_cols":17,"rows_kept":27,"cut":false,"hidden":false,"merged":[[1,16,3,17]]}
[null,0.19120872989633655,-8.5258054180521068]
[null,0.19120872989633655,-8.5258054180521068,null,null,null,null,null,null,null,2,null,null,null,null,null,"Méthode d'obtention des phaseurs initaux à partir des composantes symétriques\ncomposante homopolaire"]
[null,0.19120872989633655,-8.5258054180521068]
["Homopolaire","Ampl","Angle",null,0.01]
[null,0.19120872989633655,-8.5258054180521068,0,1,{"$f":"E5*(D5*G15-IF(D5>0,0,E4*SIN(C5*PI()/180)))","v":1.4825483849287527E-3},{"$f":"E5*($B5*COS($C5/180*PI())+F5)","v":0.19057826717482793},{"$f":"E5*(D5*I15+IF(D5>0,0,E4*COS(C5*PI()/180)))","v":9.8894919124465214E-3},{"$f":"E5*($B5*SIN($C5/180*PI())+H5)","v":-1.8458127456762664E-2},null,0,0,{"$f":"G8*$K5","v":0},0,{"$f":"I8*$K5","v":0}]
[null,0.19120872989633655,-8.5258054180521068,0,1,{"$f":"E6*D6*G16","v":0},{"$f":"E6*($B6*COS($C6/180*PI())+F6)","v":0.18909571878989917},{"$f":"E6*D6*I16","v":0},{"$f":"E6*($B6*SIN($C6/180*PI())+H6)","v":-2.8347619369209185E-2},{"$f":"1/INT(SQRT(G6^2+I6^2)/0.1)","v":1},0,0,{"$f":"G9*$K6","v":0},0,{"$f":"I9*$K6","v":0}]
[null,0.19120872989633655,-8.5258054180521068,0,1,{"$f":"E7*(D7*G17+IF(D7>0,0,E4*SIN(C5*PI()/180)))","v":-1.4825483849287527E-3},{"$f":"E7*($B7*COS($C7/180*PI())+F7)","v":0.18761317040497041},{"$f":"E7*(D7*I17-IF(D7>0,0,E4*COS(C5*PI()/180)))","v":-9.8894919124465214E-3},{"$f":"E7*($B7*SIN($C7/180*PI())+H7)","v":-3.8237111281655703E-2},null,0,0,0,0,0,null,{"$f":"IF($K$2=1,\"ð\",\"\")","v":""}]
[null,null,null,null,null,null,0.9961946980917451,null,6.3561456807761402E-2]
[null,null,null,null,null,null,-0.27361611466053531,null,-0.7517540966287265]
[null,null,null,null,null,null,-0.15529142706151239,null,0.57955549577344134,null,null,null,null,null,null,null,{"$f":"IF($K$2=2,\"ð\",\"\")","v":"ð"}]
[null,9.3899980509878772E-2,78.180464332165784]
[null,9.3899980509878772E-2,198.1804643321658]
[null,9.3899980509878772E-2,318.1804643321658,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($K$2=3,\"ð\",\"\")","v":""}]
["Inverse","Ampl","Angle"]
[null,9.3899980509878772E-2,78.180464332165784,0,1,{"$f":"E15*D15*G25","v":0},{"$f":"E15*($B15*COS($C15/180*PI())+F15)","v":1.9233513876861646E-2},{"$f":"E15*D15*I25","v":0},{"$f":"E15*($B15*SIN($C15/180*PI()))","v":9.1909076176970597E-2}]
[null,9.3899980509878772E-2,198.1804643321658,0,1,{"$f":"E16*D16*G26","v":0},{"$f":"E16*($B16*COS($C16/180*PI())+F16)","v":-8.9212351746046498E-2},{"$f":"E16*D16*I26","v":0},{"$f":"E16*($B16*SIN($C16/180*PI())+H16)","v":-2.9297826467082604E-2},null,null,null,null,null,null,null,{"$f":"IF($K$2=4,\"ð\",\"\")","v":""}]
[null,9.3899980509878772E-2,318.1804643321658,0,1,{"$f":"E17*D17*G27","v":0},{"$f":"E17*($B17*COS($C17/180*PI())+F17)","v":6.9978837869184865E-2},{"$f":"E17*D17*I27","v":0},{"$f":"E17*($B17*SIN($C17/180*PI())+H17)","v":-6.2611249709888017E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($K$2=5,\"ð\",\"\")","v":""}]
[]
[]
[null,0.78821867647140975,1.7153297798986948]
[null,0.78821867647140975,241.7153297798987]
[null,0.78821867647140975,121.7153297798987]
["Directe","Ampl","Angle"]
[null,0.78821867647140975,1.7153297798986948,null,1,0,{"$f":"IF(E25=2,G8,E25*$B25*COS($C25/180*PI()))","v":0.78786546542498448},0,{"$f":"IF(E25=2,I8,E25*$B25*SIN($C25/180*PI()))","v":2.3594285939896549E-2}]
[null,0.78821867647140975,241.7153297798987,null,1,0,{"$f":"IF(E26=2,G9,E26*($B26*COS($C26/180*PI())+F26))","v":-0.37349948170438807},0,{"$f":"IF(E26=2,I9,E26*($B26*SIN($C26/180*PI())+H26))","v":-0.694108650792435}]
[null,0.78821867647140975,121.7153297798987,null,1,0,{"$f":"IF(E27=2,G10,E27*($B27*COS($C27/180*PI())+F27))","v":-0.41436598372059652},0,{"$f":"IF(E27=2,I10,E27*($B27*SIN($C27/180*PI())+H27))","v":0.67051436485253868}]