{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Form d'Euler"],"not_rendered":{"charts":1,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Form d'Euler","index":0,"n_rows":26,"n_cols":14,"rows_kept":26,"cut":false,"hidden":false,"merged":[[20,13,22,16],[12,2,12,3],[16,3,16,4],[12,4,12,5],[16,1,16,2],[3,2,3,3],[7,2,7,5],[8,2,8,3],[8,4,8,5],[3,4,3,5]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Animation montrant le principe de la formule d'Euler :"]
[]
[null,null,"Vecteur tournant",null,"Projection horizontale"]
[null,null,0,0,{"$f":"MIN(0,C6)","v":0},{"$f":"D6","v":1},null,1.4,1.4]
[null,0,{"$f":"COS(B6+PI()/2)","v":6.1257422745431001E-17},{"$f":"SIN(B6+PI()/2)","v":1},{"$f":"B6+1.4","v":1.4},{"$f":"D6","v":1},null,1.4,-1.4]
[]
[null,null,"Projection réelle du vecteur tournant",null,null,null,null,{"$f":"PI()/2+1.4","v":2.9707963267948965},0.03]
[null,null,"graphe tournant",null,"graphe cosinus",null,null,{"$f":"H8","v":2.9707963267948965},-0.03]
[null,null,0,{"$f":"F10","v":1},{"$f":"B6+1.4","v":1.4},{"$f":"F6","v":1}]
[null,null,0,{"$f":"F11","v":0},{"$f":"B6+1.4","v":1.4},0,null,{"$f":"PI()+1.4","v":4.5415926535897935},0.03]
[null,null,null,null,null,null,null,{"$f":"H11","v":4.5415926535897935},-0.03]
[null,null,"θ tournant",null,"θ cosinus"]
[null,null,{"$f":"COS((B6/2+PI()/2))*0.35-0.09","v":-8.9999999999999969E-2},{"$f":"SIN((B6/2+PI()/2))*0.35+0.03","v":0.38},{"$f":"B6/2+1.4","v":1.4},-0.1,null,{"$f":"3*PI()/2+1.4","v":6.11238898038469},0.03]
[null,null,null,null,null,null,null,{"$f":"H14","v":6.11238898038469},-0.03]
[]
[null,"Cosinus",null,"angle tournant",null,"angle cosinus",null,{"$f":"2*PI()+1.4","v":7.6831853071795866},0.03]
[null,null,null,null,null,null,null,{"$f":"H17","v":7.6831853071795866},-0.03]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"À noter que pour les fins de cette animation l'axe des réels ℝ est ici tourné de 90° anti-horaire"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Pour les fins du cours \"Caractéristiques électriques des postes HT/MT\""]